500 Series

CM500 series

1. CE mark, fire rated

2. EN1125 and EN1634 approved

3. None handed

4. Pullman latch and lateral latch design

6. Modular design, more than 4 point locks are available 7. Material: stainless steel or steel powder coating

8. Difference finish is available

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Category of use | Durability | Door Mass | Suitability for use on | Safety fire/smoke doors | Corrosion resistance | Security | Project of horizontal bar | Type of horizontalbar operation | Field of Door application |
| 3 | 7 | 6 | B | 1 | 4 | 2 | 2 | A | A |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | ER-CM501 | ER-CM505 | ER-CM506 | ER-CM507 | ER-CM508 | ER-CM509 | ER-CM510 | ER-CM511 |
| Lock Point | 1 | 1 | 2 | 2 | 3 | 4 | 3 | 4 |
| Push Bar | 1,000mm length |
| Door Style | Single and double door | Single door | Single and double door |
| Max. Door Weight | 200kg. |
| Dogging Device | N/A |
| Security Anti-thrust latch | N/A |
| Door Width\* | up to 1,500mm |
| Door Height\* | 2,133mm |
| Door thickness\* | 50mm |

\*Note: if the door width, door height and door thickness is outside of the specification, the order should mark the special requirement.

FOB Kaohsiung, Taiwan

T/T Payment

MOQ 84 sets